국 문 규 격 서

COMMODITY DESCRIPTION

관세분류 번호 HSK No.	픔목번호 Item No.	품명 및 규격	규 격 Unit	수 량 Quantity
9016002000	MB45	수분 분석기	Set	1

A. Feature

1. 기존의 적외선 건조방식보다 40%이상 빠르게 가열하는 할로겐 전극은 섭씨 200도 까지 균일하게 가열.

2. 통합 데이터 베이스로 50개까지 건조분석 과정을 저장하고 불러낼 수 있는 기능.

3. 작동, 데이터 저장, 사용자 맞춤 작업이 용이하도록 설계된 강력한 소프트웨어.

4. %수분도, %고형도, 무게, 온도, 시간, 실시간 건조 곡선 등이 표시되는 디스플레이.

5. GLP 인쇄를 위한 RS232 Output - 결과, 시간/날짜, ID 인쇄.

6. 간단한 소프트웨어 조작으로 쉽게 할 수 있는 테스트 파라미터 셋업.

7. 최적의 성능과 속도를 위한 사용자선택 자동 꺼짐 기능.

B. Specification

1. Capacity : 45 g

2. Readability : 0.01 %/0.001 g

3. Repeatibility (Std. Dev.) : 0.05% (3g sample)/0.015%(10g sample)

4. Moisture range : 0.01% to 100%

5. Timer : 1 - 120 minutes

6. Heat source : Halogen

7. Temperature settings : 50° to 200° in 1°C increments

8. Stabilization time (seconds): 3

9. Operating Temperature Range: 50° to 104°F / 10° to 40°C

10. Tare range : To capacity by subtraction

11. Display Type: 128 x 64 pixel graphical backlit LCD display

12. Pan size (in/mm): 3.54 / 90

13. Dimensions WxHxD (in/cm): 7.5 x 6 x 14.2 / 19 x 15.2 x 36

C. Optional Accessories

* OH-380D Printer / RS232 Cable

* Balance Talk Software

D. Remarks