국 문 규 격 서

COMMODITY DESCRIPTION

관세분류 번호 HSK No.	픔목번호 Item No.	품명 및 규격	규 격 Unit	수 량 Quantity
9016002000	AVG413C	정밀용 저울	Set	1

A. Feature

1. 사용자와 저울간의 인터페이스 최적의 조건을 만드는 4버튼 간편 작동법

2. 한층 강화된 부품수 카운팅, 저울 밑 무게측정 동물계량, 무게검수, 백분율, 총계, 화면캡처

3. 다양한 계측단위

4. 밀도/비중 측정이 가능

5. RS232를 사용한 GLP 인쇄 - 실험결과, 시간/날짜. ID, 캘리브레이션 내용 인쇄.

6. 날짜, 시간, 저울 시리얼 넘버, 사용자, 프로젝트명, 실험결과 등을 완벽하게 나타낼 수 있는 대용량 GLP/GMP

7. 분동 내장형

B. Specification

1. Capacity : 410 g

2. Readability : 0.001 g

3. Repeatibility (Std. Dev.) : 0.001 g

4. Linearity : ±0.002

5. Weighing units : Milligram, gram, kilogram, carat

6. Application Modes: Weighing, Dynamic Weighing, Parts Counting with Automatic Sample                                         Recalibration, Percent Weighing, Checkweighing, Totalization, Display Hold

7. Tare range: To capacity by subtraction

8. Stabilization time (seconds): 3

9. Operating Temperature Range: 50° to 86° F / 10° to 30° C

10. Calibration: Digital with Internal Weight

11. Display type: 2-Line Alphanumeric Brilliant Backlit LCD Display With Text Prompts

12. Display (in/cm): 4 x 1 / 10 x 2.5

13. Pan size (in/cm): 4.7 / 12

14. Dimensions WxHxD (in/cm): 8.7 x 7.5 x 11.8 / 22 x 19 x 30(with draft shield)

C. Optional Accessories

* OH-380D Printer / RS232 Cable

* Balance Talk Software

D. Remarks