국 문 규 격 서

COMMODITY DESCRIPTION

관세분류 번호 HSK No.	픔목번호 Item No.	품명 및 규격	규 격 Unit	수 량 Quantity
9016002000	SPG2001F	정밀용 저울	Set	1

A. Feature

1. 조작이 간단하며 최소한의 동작으로 무게측정이 가능하며 응용기능의 업그레이드로 향상된 분석력을 제공합니다

2. grams, kilograms 등 다양한 계측단위

3. 강화된 부품수 카운팅 기능, 백분율(%), 총계, 디스플레이 홀드 등 다양한 기능모드

4. 고해상도 LCD 디스플레이와 2 버튼 작동 시스템이 조화되어 스카우트 프로의 작동법을 간단하고 쉽게 만들어 준다.

5. 즉시 설치 옵션으로 케이블을 통하여 PC 또는 프린터와의 연결을 가능하게 한다.

6. 청소를 위한 해체가 간편한 짐판, 앞판넬로 철저히 봉인된 표시부와 오물 방지용 홈은 스카우트 프로를 각종 오물과 먼지로부터 안전하고 청결하게 지켜준다.

7. 4“AA" 베터리(40시간 작동을 위한 작동 전원 차단장치)와 AC 어댑터 겸용으로 사용 가능

8. 밀도 및 비중 측정분석이 가능한 저울밑 무게 측정 고리

B. Specification

1. Capacity (metric): 2000 g

2. Readability (metric): 0.1 g

3. Repeatibility (Std. Dev.) (g): 0.1

4. Linearity (g): ±0.1

5. Application Modes: Parts Counting with Average Piece Weigh Recalculation, Percentage Weighing, Totalization, Display Hold

6. Tare range: To capacity by subtraction

7. Over range capacity: Capacity +90d

8. Stabilization time (seconds): 3

9. Operating temperature range: 50° to 104°F / 10° to 40°C

10. Power requirements: AC Adapter (included) or 4 AA Batteries (not included)

11. Calibration: Digital calibration from keypad

12. Display: High Contrast LCD with 6 digits 0.6in/15mm high

13. Pan size (in/cm): 6.5 x 5.5 / 16.5 x 14.2

14. Dimensions WxHxD (in/cm): 7.56 x 2.13 x 8.27 / 19.2 x 5.4 x 21

c. Remarks